ZEU Radio Frequencies and Channels

for Baofeng Radios

Date Revised: ‎2016-‎01-‎10 ZEU Team Channels

Channel Name/ Frequency Name Channel Frequency

|  |  |
| --- | --- |
| ZC 1 (MURS CH 1) | 151.8200 |
| ZC 2 (MURS CH 2) | 151.8800 |
| ZC 3 (MURS CH 3) | 151.9400 |
| ZC 4 (MURS CH 4) | 154.5700 |
| ZC 5 (MURS CH 5) | 154.6000 |
| ZC 6 [Vehicle-to-Vehicle Only] (Open - No Frequency) |  |
| ZC 7 [Vehicle-to-Leaders Only] (Open - No Frequency) |  |

FRS/GMRS Channels

Channel Name/Frequency Name Channel Frequency

|  |  |
| --- | --- |
| FRS1 (FRS/GMRS CH 1) | 462.5625 |
| FRS2 (FRS/GMRS CH 2) | 462.5875 |
| FRS3 (FRS/GMRS CH 3) | 462.6125 |
| FRS4 (FRS/GMRS CH 4) | 462.6275 |
| FRS5 (FRS/GMRS CH 5) | 462.6625 |
| FRS6 (FRS/GMRS CH 6) | 462.6875 |
| FRS7 (FRS/GMRS CH 7) | 462.7125 |
| FRS8 (FRS/GMRS CH 8) | 467.5625 |
| FRS9 (FRS/GMRS CH 9) | 467.5875 |
| FRS10 (FRS/GMRS CH 10) | 467.6125 |
| FRS11 (FRS/GMRS CH 11) | 467.6375 |
| FRS12 (FRS/GMRS CH 12) | 467.6625 |
| FRS13 (FRS/GMRS CH 13) | 467.6875 |
| FRS14 (FRS/GMRS CH 14) | 467.7125 |
| FRS15 (FRS/GMRS CH 15) | 462.5500 |
| FRS16 (FRS/GMRS CH 16) | 462.5750 |
| FRS17 (FRS/GMRS CH 17) | 462.6000 |
| FRS18 (FRS/GMRS CH 18) | 462.6250 |
| FRS19 (FRS/GMRS CH 19) | 462.6500 |
| FRS20 (FRS/GMRS CH 20) | 462.6750 |
| FRS21 (FRS/GMRS CH 21) | 462.7000 |
| FRS22 (FRS/GMRS CH 22) | 462.7250 |

National Weather Service Channels

Channel Name/Location Channel Frequency/Power

|  |  |
| --- | --- |
| LYONS (NOAA Lyons, NY) | 162.4750 (250W) |
| ROCH (NOAA Rochester, NY) | 162.4000 (500W) |